| CY8CKIT-041S-MAX BSP

Macros
Pin States

## General Description

Macros to abstract out whether the LEDs & Buttons are wired high or active low.

Copyright
  Copyright 2018-2022 Cypress Semiconductor Corporation (an Infineon company) or an affiliate of Cypress Semiconductor Corporation

SPDX-License-Identifier: Apache-2.0

Licensed under the Apache License, Version 2.0 (the "License"); you may not use this file except in compliance with the License. You may obtain a copy of the License at

    http://www.apache.org/licenses/LICENSE-2.0

Unless required by applicable law or agreed to in writing, software distributed under the License is distributed on an "AS IS" BASIS, WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied. See the License for the specific language governing permissions and limitations under the License.

## Macros
#define | CYBSP_LED_STATE_ON (0U)
| Pin state for the LED on.
#define | CYBSP_LED_STATE_OFF (1U)
| Pin state for the LED off.
#define | CYBSP_BTN_PRESSED (0U)
| Pin state for when a button is pressed.
#define | CYBSP_BTN_OFF (1U)
| Pin state for when a button is released.