| CY8CKIT-041S-MAX BSP

Functions
Functions

## General Description

All functions exposed by the board.

## Functions
cy_rslt_t | cybsp_init (void)
| Initialize all hardware on the board. More...

## Function Documentation

## ◆ cybsp_init()

cy_rslt_t cybsp_init | ( | void |  | ) |

Initialize all hardware on the board.

Returns
  CY_RSLT_SUCCESS if the board is successfully initialized, if there is a problem initializing any hardware it returns an error code specific to the hardware module that had a problem.