| CY8CKIT-041S-MAX BSP

API Reference
Pin Mappings

## General Description

Macro definitions for common peripheral pins on the board.

Copyright
  Copyright 2018-2022 Cypress Semiconductor Corporation (an Infineon company) or an affiliate of Cypress Semiconductor Corporation

SPDX-License-Identifier: Apache-2.0

Licensed under the Apache License, Version 2.0 (the "License"); you may not use this file except in compliance with the License. You may obtain a copy of the License at

    http://www.apache.org/licenses/LICENSE-2.0

Unless required by applicable law or agreed to in writing, software distributed under the License is distributed on an "AS IS" BASIS, WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied. See the License for the specific language governing permissions and limitations under the License.

## API Reference
| LED Pins
| Pins connected to user LEDs on the board.
| Button Pins
| Pins connected to user buttons on the board.
| Communication Pins
| Pins associated with connections on the board for communication interfaces (UART/I2C/SPI/...)
| Arduino Header Pins
| Pins mapped to the Arduino header on the board.
| J2 Header Pins
| Pins mapped to the J2 header on the board.